**REGISTRATION OF PETROL PUMP IN AJ&K**

**DOCUMENTS REQUIRED FOR Petrol pump**

1. Application for availability of name will be sent to Registrar, Deputy Registrar of Firms.
2. Six Copies of Plan from Oil Marketing Company one copy must be signed by the Deputy Commissioner.
3. Form D Petrol / Desil from Company.
4. Attested copy of Agreement between Company and Dealer Petrol pump.
5. Original NOC from Deputy Commissioner relevant District.
6. Attested copies of NOC from the Department of PWD road Division, Electricity, Public Health, Telecommunication Organization, Muncipal Corporation & Defense.
7. Documents
8. Attested copies of CNIC Dealer Petrol Pump

**Required Documents for grant of Petroleum License in Form “K”**

1. Application form “D” duly filled in any signed.
2. Treasury Challan for grant of license.
3. Original NOC issued by concerned District Authority along with site plan showing dimensions of plot attested by him.
4. Copy of valid registered land lease agreement between owner of land and Oil Marketing Company.
5. Six sets of proposed plans showing installation of equipment according to Petroleum Rules, 1937.
6. The site shall not be located in a narrow street to cause congestion and interference with the flow of traffic.
7. The Petrol pump site shall be suitably located to given service to the motorist where be most needs it. It should be visible from a distance and easily accessible.
8. Petrol pump shall be well away from tramway lines, bridges and bridge approaches.
9. Front Pump Island shall be at least 20 meters away from the point where center lines of two roads meet each other, and 4 meters inside from the front boundary line of the premises.
10. Every site shall have a minimum frontage of 23 meters and depth 14 meters, not including pavements area of a road to permit construction of kiosk/service station, except a corner site of “Y” shape forming a triangle at the junction of 3 roads which may be approved irrespective of its size for the barest fuelling facilities.
11. The site shall be located at least 7 meter away from a public bust parking place and be capable of being a fenced off with a boundary wall.